<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<library>
<packages>
<package name="TSSOP24">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 24&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="TSSOP28">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 28&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
</packages>
<symbols>
<symbol name="TLC5925">
<description>TLC5925 Constant Current Shift register</description>
<pin name="GND" direction="sup"/>
<pin name="VDD" direction="pwr"/>
<pin name="R-EXT" direction="pas"/>
<pin name="SDI" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="SDO" direction="out"/>
<pin name="LE" direction="in"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="OUT0" direction="out" function="dot"/>
<pin name="OUT1" direction="out" function="dot"/>
<pin name="OUT2" direction="out" function="dot"/>
<pin name="OUT3" direction="out" function="dot"/>
<pin name="OUT4" direction="out" function="dot"/>
<pin name="OUT5" direction="out" function="dot"/>
<pin name="OUT6" direction="out" function="dot"/>
<pin name="OUT7" direction="out" function="dot"/>
<pin name="OUT8" direction="out" function="dot"/>
<pin name="OUT9" direction="out" function="dot"/>
<pin name="OUT10" direction="out" function="dot"/>
<pin name="OUT11" direction="out" function="dot"/>
<pin name="OUT12" direction="out" function="dot"/>
<pin name="OUT13" direction="out" function="dot"/>
<pin name="OUT14" direction="out" function="dot"/>
<pin name="OUT15" direction="out" function="dot"/>
</symbol>
<symbol name="FT260">
<description>HID-class USB to UART/I2C
Bridge IC</description>
<pin name="FSOURCE" direction="pwr"/>
<pin name="VBUS_DET" direction="in"/>
<pin name="DIO12"/>
<pin name="DIO13"/>
<pin name="DEBUGGER" direction="in"/>
<pin name="STEST_RSTN" direction="in"/>
<pin name="RESETN" direction="in"/>
<pin name="DCNF0" direction="in"/>
<pin name="DCNF1" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="DIO0"/>
<pin name="DIO1"/>
<pin name="DIO2"/>
<pin name="DIO3"/>
<pin name="AGND" direction="sup"/>
<pin name="VCCIN" direction="pwr"/>
<pin name="VOUT3V3" direction="pwr"/>
<pin name="DP"/>
<pin name="DM"/>
<pin name="GND" direction="sup"/>
<pin name="DIO11"/>
<pin name="DIO10"/>
<pin name="DIO9"/>
<pin name="DIO8"/>
<pin name="DIO7"/>
<pin name="DIO6"/>
<pin name="DIO5"/>
<pin name="DIO4"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TLC5925">
<gates>
<gate name="G$1" symbol="TLC5925"/>
</gates>
<devices>
<device name="IPWR" package="TSSOP24">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LE" pad="4"/>
<connect gate="G$1" pin="OE" pad="16"/>
<connect gate="G$1" pin="OUT0" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT10" pad="22"/>
<connect gate="G$1" pin="OUT11" pad="21"/>
<connect gate="G$1" pin="OUT12" pad="20"/>
<connect gate="G$1" pin="OUT13" pad="19"/>
<connect gate="G$1" pin="OUT14" pad="18"/>
<connect gate="G$1" pin="OUT15" pad="17"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="9"/>
<connect gate="G$1" pin="OUT5" pad="10"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="12"/>
<connect gate="G$1" pin="OUT8" pad="24"/>
<connect gate="G$1" pin="OUT9" pad="23"/>
<connect gate="G$1" pin="R-EXT" pad="14"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="15"/>
<connect gate="G$1" pin="VDD" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT260">
<description>USB HID to UART/I2C bridge</description>
<gates>
<gate name="G$1" symbol="FT260"/>
</gates>
<devices>
<device name="S-U" package="TSSOP28">
<connects>
<connect gate="G$1" pin="AGND" pad="15"/>
<connect gate="G$1" pin="DCNF0" pad="8"/>
<connect gate="G$1" pin="DCNF1" pad="9"/>
<connect gate="G$1" pin="DEBUGGER" pad="5"/>
<connect gate="G$1" pin="DIO0" pad="11"/>
<connect gate="G$1" pin="DIO1" pad="12"/>
<connect gate="G$1" pin="DIO10" pad="22"/>
<connect gate="G$1" pin="DIO11" pad="21"/>
<connect gate="G$1" pin="DIO12" pad="3"/>
<connect gate="G$1" pin="DIO13" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="13"/>
<connect gate="G$1" pin="DIO3" pad="14"/>
<connect gate="G$1" pin="DIO4" pad="28"/>
<connect gate="G$1" pin="DIO5" pad="27"/>
<connect gate="G$1" pin="DIO6" pad="26"/>
<connect gate="G$1" pin="DIO7" pad="25"/>
<connect gate="G$1" pin="DIO8" pad="24"/>
<connect gate="G$1" pin="DIO9" pad="23"/>
<connect gate="G$1" pin="DM" pad="19"/>
<connect gate="G$1" pin="DP" pad="18"/>
<connect gate="G$1" pin="FSOURCE" pad="1"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="RESETN" pad="7"/>
<connect gate="G$1" pin="STEST_RSTN" pad="6"/>
<connect gate="G$1" pin="VBUS_DET" pad="2"/>
<connect gate="G$1" pin="VCCIN" pad="16"/>
<connect gate="G$1" pin="VCCIO" pad="10"/>
<connect gate="G$1" pin="VOUT3V3" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
